**Convert to PV-GRUB …**

|  |  |  |
| --- | --- | --- |
| If the ROOT disk have … | No Partition ( /dev/sdx ) | Partitions ( /dev/sdx*n* ) |
| Use compatible PV-GRUB's AKI …  Do not use ARI … | us-east-1  aki-88aa75e1 pv-grub-hd0\_1.03-x86\_64.gz  aki-b6aa75df pv-grub-hd0\_1.03-i386.gz  us-west-1  aki-f77e26b2 pv-grub-hd0\_1.03-x86\_64.gz  aki-f57e26b0 pv-grub-hd0\_1.03-i386.gz  us-west-2  aki-fc37bacc pv-grub-hd0\_1.03-x86\_64.gz  aki-fa37baca pv-grub-hd0\_1.03-i386.gz  eu-west-1  aki-71665e05 pv-grub-hd0\_1.03-x86\_64.gz  aki-75665e01 pv-grub-hd0\_1.03-i386.gz  ap-southeast-1  aki-fe1354ac pv-grub-hd0\_1.03-x86\_64.gz  aki-f81354aa pv-grub-hd0\_1.03-i386.gz  ap-southeast-2  aki-33990e09 pv-grub-hd0\_1.03-i386.gz  aki-31990e0b pv-grub-hd0\_1.03-x86\_64.gz | us-east-1  aki-b4aa75dd pv-grub-hd00\_1.03-x86\_64.gz  aki-b2aa75db pv-grub-hd00\_1.03-i386.gz  us-west-1  aki-eb7e26ae pv-grub-hd00\_1.03-x86\_64.gz  aki-e97e26ac pv-grub-hd00\_1.03-i386.gz  us-west-2  aki-f837bac8 pv-grub-hd00\_1.03-x86\_64.gz  aki-f637bac6 pv-grub-hd00\_1.03-i386.gz  eu-west-1  aki-8b655dff pv-grub-hd00\_1.03-x86\_64.gz  aki-89655dfd pv-grub-hd00\_1.03-i386.gz  ap-southeast-1  aki-fa1354a8 pv-grub-hd00\_1.03-x86\_64.gz  aki-f41354a6 pv-grub-hd00\_1.03-i386.gz  ap-southeast-2  aki-3f990e05 pv-grub-hd00\_1.03-i386.gz  aki-3d990e07 pv-grub-hd00\_1.03-x86\_64.gz |
| Attach EBS disk as … | /dev/sda1 | /dev/sda |
| Populate /boot … | … with the desired kernel version … | … with the desired kernel version … |
| Configure /boot/grub/menu.lst … | default 0  timeout 1  title My Linux Server (version)  root (hd0)  kernel /boot/vmlinuz-version ro root=/dev/sda1  initrd /boot/initrd-version.img | default 0  timeout 1  title Oracle Linux Server (version)  root (hd0,0)  kernel /boot/vmlinuz-version ro root=/dev/sda1  initrd /boot/initrd-version.img |